Operation void setAlarmReportingOn (), in Class EquipmentHolder

Documentation
This operation allows (activates, or turns on) alarm reporting on this equipment holder.
Note: If alarm monitoring is enabled, this does not mean that alarm is reported anyway, because Alarm Severity Assignment Profile may perform further filtering.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when alarm reporting can not be enabled.
4. NE_COMM_LOSS - Raised when communication to the managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
Alarm monitoring is enabled on the equipment holder.
Semantics