This operation allows an NMS to request all of the equipments that supports the equipment, e.g., the power pack and synchronization card that support a given piece of equipment.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.
