CIS Boolean edgePoint = NA, in Class TerminationPoint

Documentation
Indicates if the TP is an edge point of at least one subnetwork, i.e. if it is an end point of a potential inter-subnetwork topological link.
Changes in the value of this attribute lead to a AVC notification.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? No

Export Control | PublicAccess | Containment | Unspecified
Static | No | Derived | No