Indicates the external traffic flow of the requested subnetwork connection through the subnetwork.
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
