tmf854.v1 > ESwitchReason_T LOCATION: file:/xsd/networkResources/GlobalDefinitions.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The ESwitchReason_T Simple Type
The equipment switch reason reflects the reason why a switch occurred. EswitchReason is a string that can take the following values.
Simple Type ESwitchReason_T
ESwitchReason_T is union of (string, string, string).
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*`".
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`PROP_([a-z]|[A-Z]|[0-9]|(_|-))*`".
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are

Enumeration | Description
SR_NA | It is used, if a more precise value is not available.
SR_E_FAILURE | It is used when an instance of equipment has failed.
SR_MANUAL | It indicates a switch that was requested by the operator and includes forced switches.

(SR_NA | SR_E_FAILURE | SR_MANUAL).

XML
-<xsd:simpleType name="ESwitchReason_T"> -<xsd:annotation> <xsd:documentation> The equipment switch reason reflects the reason why a switch occurred. EswitchReason is a string that can take the following values. </xsd:documentation> </xsd:annotation> -<xsd:union> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:pattern value="MINOR_([a-z]|[A-Z]|[0-9]|(_|-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:pattern value="PROP_([a-z]|[A-Z]|[0-9]|(_|-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> -<xsd:enumeration value="SR_NA"> -<xsd:annotation> <xsd:documentation> It is used, if a more precise value is not available. </xsd:documentation> </xsd:annotation> </xsd:enumeration> -<xsd:enumeration value="SR_E_FAILURE"> -<xsd:annotation> <xsd:documentation> It is used when an instance of equipment has failed. </xsd:documentation> </xsd:annotation> </xsd:enumeration> -<xsd:enumeration value="SR_MANUAL"> -<xsd:annotation> <xsd:documentation> It indicates a switch that was requested by the operator and includes forced switches. </xsd:documentation> </xsd:annotation> </xsd:enumeration> </xsd:restriction> </xsd:simpleType> </xsd:union> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (2) EProtectionSwitch_T/eSwitchReason ESwitchData_T/eSwitchReason

Generated by WSDLdoc ©