Operation void getAllFixedCrossConnections (CIS SequenceOf Enums::LayerRate connectionRateList = NA, CIS SequenceOf CrossConnection crossConnections = NA), in Class ManagedElement

Documentation
This operation allows an NMS to request a list of the fixed cross-connects for the specified managed element at the specified layer rates.
The operation will also return fixed cross connections between GTPs.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when connectionRateList is empty or contains invalid rates.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

connectionRateList
/* in */ List of rates for which to retrieve the fixed cross-connections. This must not be an empty list. In this case an INVALID_INPUT exception is thrown.
crossConnections
/* out */ The fixed cross-connections matching the specified layer rate(s).