SNCState sncState = NA, in Class SubnetworkConnection

Documentation
The SNC connection state.
Changes in the value of this attribute lead to a State Change notification.
Possible values are:
- PENDING: the SNC has been created by an NMS and has not been activated by any NMS; or the SNC has been successfully deactivated by an NMS. That state has no relationship with the network state of the cross-connects of the SNC.
-
ACTIVE: the SNC is not in pending state, a route has been assigned to the SNC and all cross-connects for the SNC are active in the network.
- PARTIAL: the SNC is not in pending state, and either a route has not been assigned to the SNC, or not all of the cross-connects of the SNC are active in the network. This may or may not include activated SNCs for which there are currently no active cross-connects in the network, depending on the SNC management mode of operation.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No