Represents a static, inherent capability of the TP. This is not a dynamic state/status indication.
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
