tmf854.v1 > ActiveAlarmFilter_T LOCATION: file:/xsd/interfaces/AlarmRetrieval.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The ActiveAlarmFilter_T Complex Type
The active alarm filter data structure. Default interpretation (filter criteria is missing or is an empty list) indicates that it is not relevant to the query. All the filter criteria possible enumerations are applicable. Examples: #1: All filter criteria missing -> Retrieve all alarms associated with all MEs and this OS #2: source=internal, all other criteria missing -> Retrieve all alarms associated with this OS only #3: source=external, all other criteria missing -> Retrieve all alarms associated with the MEs only

Local elements (5)
  source scope perceivedSeverityList probableCauseList acknowledgeIndication

Complex Type ActiveAlarmFilter_T
The ActiveAlarmFilter_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> -Begin Sequence [1...1] This attribute filters the alarms based on their source (with respect to the OS receiving this request). Possible values are INTERNAL, EXTERNAL, NOT_APPLICABLE. The value NOT_APPLICABLE means there is no filtering on the alarm source; i.e., internal and external alarms are in the scope. <source>AlarmSource_T</source> [0..1] This attribute filters the alarms based on a list of managed elements. The listed managed elements are in the scope. If no managed element is provided, alarms from all managed elements are in scope. <scope extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributesList_T</scope> [0..1] This attribute filters the alarms based on a list of severities (see ITU-T X.733 definitions). The listed severities are in the scope. If no severity is provided, alarms with any severity are in scope. <perceivedSeverityList>PerceivedSeverityList_T</perceivedSeverityList> [0..1] This attribute filters the alarms based on a list of probable causes (for details refer to the supporting document: ProbableCauses). The listed probable causes are in the scope. If no probable cause is provided, alarms with any probable cause are in scope. <probableCauseList extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">ProbableCauseList_T</probableCauseList> [0..1] This attribute filters the alarms based on its acknowledge indication. Possible values are EVENT_ACKNOWLEDGED, EVENT_UNACKNOWLEDGED, and NOT_APPLICABLE. The value NOT_APPLICABLE indicates that alarms with any acknowledge indication are in scope. <acknowledgeIndication>AcknowledgeIndication_T</acknowledgeIndication> [0..1] End Sequence </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:complexType name="ActiveAlarmFilter_T"> -<xsd:annotation> <xsd:documentation> The active alarm filter data structure. Default interpretation (filter criteria is missing or is an empty list) indicates that it is not relevant to the query. All the filter criteria possible enumerations are applicable. Examples: #1: All filter criteria missing -> Retrieve all alarms associated with all MEs and this OS #2: source=internal, all other criteria missing -> Retrieve all alarms associated with this OS only #3: source=external, all other criteria missing -> Retrieve all alarms associated with the MEs only </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element minOccurs="0" name="source" type="AlarmSource_T"> -<xsd:annotation> <xsd:documentation> This attribute filters the alarms based on their source (with respect to the OS receiving this request). Possible values are INTERNAL, EXTERNAL, NOT_APPLICABLE. The value NOT_APPLICABLE means there is no filtering on the alarm source; i.e., internal and external alarms are in the scope. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="scope" type="NamingAttributesList_T"> -<xsd:annotation> <xsd:documentation> This attribute filters the alarms based on a list of managed elements. The listed managed elements are in the scope. If no managed element is provided, alarms from all managed elements are in scope. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="perceivedSeverityList" type="PerceivedSeverityList_T"> -<xsd:annotation> <xsd:documentation> This attribute filters the alarms based on a list of severities (see ITU-T X.733 definitions). The listed severities are in the scope. If no severity is provided, alarms with any severity are in scope. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="probableCauseList" type="ProbableCauseList_T"> -<xsd:annotation> <xsd:documentation> This attribute filters the alarms based on a list of probable causes (for details refer to the supporting document: ProbableCauses). The listed probable causes are in the scope. If no probable cause is provided, alarms with any probable cause are in scope. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="acknowledgeIndication" type="AcknowledgeIndication_T"> -<xsd:annotation> <xsd:documentation> This attribute filters the alarms based on its acknowledge indication. Possible values are EVENT_ACKNOWLEDGED, EVENT_UNACKNOWLEDGED, and NOT_APPLICABLE. The value NOT_APPLICABLE indicates that alarms with any acknowledge indication are in scope. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (7) AcknowledgeIndication_T AlarmSource_T NamingAttributesList_T PerceivedSeverityList_T ProbableCauseList_T string TMF854_Version_T

Used-By
Element (2) getActiveAlarms_T/filter getActiveAlarmsCount_T/filter

Generated by WSDLdoc ©