Class PmpStateChangeInformation {Analysis} derived from: Event

Documentation
This notification has to be send when PM data is cleared, PM data collection is disabled or enabled, and when TCA generation is enabled or disabled.
This notification is used to report only one type of change at a time, e.g., PM data collection is set to disable for a collection of PMPs, or TCA generation is enabled for a set of PMPs.
The EMS should not use both this notification and individual state change notifications on PMPs to report the same event. This is not to say that an EMS could not sometimes issue state change notifications on individual PMPs and other times on a list of PMPs.
Object Lifecycle: Created and deleted by EMS.
Object Creation Notification Issued? No
Object Deletion Notification Issued? No

Parent Package | Logical View | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Attributes

Name | Class | Type | Initial Value
pmpNameList | PmpStateChangeInformation | CIS SequenceOf Name |
neTime | PmpStateChangeInformation | CIS GeneralizedTime | NA
emsTime | PmpStateChangeInformation | CIS GeneralizedTime | NA
attributeList | PmpStateChangeInformation | CIS SequenceOf Structs::AVP |
notificationId | Event | CIS CharacterString | NA
eventType | Event | CIS SequenceOf CIS CharacterString | NA

Generalization Relationships

Name | Class | Supplier
--Not Named-- | PmpStateChangeInformation | Event