Operation void setNetworkAccessDomain (CIS CharcaterString networkAccessDomain = NA), in Class CommonResourceInfo

Documentation
The operation allows the NMS to change the association of the resource (which contains a networkAccessDomain attribute) to a Network Access Domain.
Operation Exceptions:
1. NOT_IMPLEMENTED - If EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when the network Access Domain attribute is not pesent in the object.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
1. The resource must contain the attribute networkAccessDomain.
2. The EMS supports setting of the Network Access Domain attribute by the NMS.
Postconditions
Network Access Domain attribute is set/modified and the corresponding AVC notification is sent.
Semantics

Arguments

networkAccessDomain
/* in */ New Network Access Domain name.