CIS CharacterString baseInstanceList = empty string, in Class InventoryFilter

Documentation
This attribute identifies a list of base object instances for the subtrees to be retrieved. BaseInstanceList is a list of serialized MTOSI names. If the BaseInstanceList is left empty then all the nodes at the top of the MTOSI instance tree are selected (i.e., all MDs, TMDs, inter-MD-TLs, and OSs are selected). Specification of the baseInstanceList does not select any objects in and of itself. In order to select specific objects, one needs to specify the IncludedObjectTypes.
The ";" is used as a separator, and "=" is used to associate a value with a type of object. For example, MD=md1;ME=ME123;EH=ACME7 identifies an equipment holder within managed element ME123 within management domain md1. The relative name of the equipment holder is ACME7.
The following abbreviations are used for the object type names:
MD - management domain
ME - managed element
EH - equipment holder
EQ - equipment
PTP - physical termination point
FTP - floating termination point
CTP - connection termination point
TPPool - termination point pool
EPGP - equipment protection group
PGP - protection group
SNC - subnetwork connection
MLSN - multi layer subnetwork
TL - topological link
OS - operations system
TMD - transmission descriptor
Readable by Requesting OS? No
Writeable by Requesting OS? Yes
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No