This operation implements the 'supports' relationship (see equipment model) between equipment and PTPs for the NMS and returns the names of PTPs only.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS- Raised when communication to managed element is lost.
