This relationship provides the list of PM parameter/threshold value pairs including location and granularity.
Changes in this relationship lead to a AVC notification issued by the TCAParameterProfile object.

Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No
