The operation verifies the egress and/or ingress TransmissionDescriptor (TMD) state of the TP.

According to the requested transmission direction it checks whether a TMD is assigned as egress and/or ingress TMD to the TP. If this is true it first verifies the existence of the assigned TMD(s) and then compares the transmission parameters of the TMD with the transmission parameters of theTP. After this the additionalTPInfo parameters of the TMD are compared with the additionalTPInfo parameters of the TP.

If a TMD transmission parameter is not present as a TP transmission parameter or is present but has a different value, this is called a "parameter mismatch", and the TMD state will take the value "mismatch".
The operation returns the current TMD state and all mismatched transmission or additionalTPInfo parameters of the TMD.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when direction value is invalid.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.
