CIS CharacterString gctHostname = NA, in Class GCTProfileInfo

Documentation
IP address (or host name which is mapped to the appropriate IP address) that allows the NMS to identify where to launch the EMS GUI client. This string can be empty only for emsGctPlatform "local" or "web-based". For Citrix commands, it is the TSE (Terminal Server Environment) IP address.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No