This attribute provides an indication of whether alarm reporting for this resource is inhibited.TRUE allowed, FALSE inhibited.
Changes in the value of this attribute lead to an AVC notification.

Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No
