The supervision state indicates whether performance threshold supervision is enabled or disabled for the PMP.
Changes in this attribute lead to a State Change notification.

Readable by NMS? Yes
Writeable by NMS? Via operations enableTCA() / disableTCA()
Invariant? No
