The attribute contains additional info parameters which can be set on a TP having this TransmissionDescriptor (TMD) assigned as egress or ingress TMD.

Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes
