Operation void getIntendedRoute (Route theRoute = NA, CIS SequenceOf Structs::AVP additionalInfo = empty list), in Class SubnetworkConnection

Documentation
The operation allows an NMS to request the intended route of the SNC.
Note: The relationship between Bundled SNC service and the SNC with Multiple Routes feature requires further study and is not applicable for v3.0.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when an EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when the EMS is unable to execute the request because at least one of the
parameters although valid can not be set and that parameter is identified as "not best effort" in additionalInfo.
If the EMS cannot determine the reason it could not comply, it is also allowed to throw UNABLE_TO_COMPLY.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

theRoute
/* out */ The intended route of the SNC.
additionalInfo
/* inout */ Allows the communication of additional information which is not explicitly modelled.