CIS Boolean alarmReportingIndication = FALSE, in Class SubnetworkConnection

Documentation
Provides an indication of whether alarm reporting for this subnetwork connection is administratively activated or de-activated.
Changes in the value of this attribute lead to a AVC notification.
True = alarm reporting is activated; False = alarm reporting is de-activated.
Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No