CIS Boolean active = NA, in Class CrossConnect

Documentation
True if the cross-connect is active in the ME; false otherwise.An "active" cross-connection means that no further intervention on the cross-connection itself is required from the NMS to activate it. The fact that a cross-connection is "active" does not necessarily imply that there is traffic flow on the network.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No