Specified by NMS upon object creation.

Note: In case of a bundled SNC the value LR_Not_Applicable is used. The NMS can determine the layerRate(s) by looking at the CTPs contained in the aEnd and zEnd GTPs.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
