Association (tpInclusions:TerminationPoint) (theSNCCreateData:SNCCreateData)

Documentation
Specifies a list of PTPs and/or CTPs that must be used by the SNC. The list must be empty if no PTP/CTP constraints are required. If the EMS cannot fully satisfy the constraints, then the request will be rejected.
Note: In case of bundled SNCs,
- for each PTP used in the inclusion list, the EMS should use a GTP that contains at least one CTP from the given PTP
- for each CTP used in the inclusion list, the EMS should use a GTP that contains the given CTP.

Derived | No | Link Class | --Not Defined--
Element 1 | TerminationPoint | Element 2 | SNCCreateData
Role 1 | tpInclusions | Role 2 | --Not Named--