Operation void getSupportedPTPs (CIS SequenceOf PhysicalTermminationPoint ptps), in Class Equipment

Documentation
This operation implements the 'supports' relationship (see equipment model) between equipment and PTPs for the NMS.This operation returns an empty list for a protecting card.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS- Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

ptps
/* out */ The PTP objects implemented on the equipment.