This attribute allows the communication from the EMS to the NMS of additional information which is not explicitly modelled.
The list may be empty.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
