Integer NEITHER_TERMINATED_NOR_AVAILABLE_FOR_MAPPING = 1, in Class TerminationMode

Documentation
The CTP can be mapped but currently is not (i.e., it does have contained potential CTPs, but currently has no contained actual CTPs). This indicates that the G.805 CP aggregated in the CTP is not connected to a TCP (that would be aggregated in the same CTP) and therefore the CTP is available for SNC/crossconnect connectivity (e.g. STS1 not terminated and not mapped to VT1.5i.e. not channelized).
The FTP can be mapped on the server side but currently is not (i.e., it does have contained potential CTPs on the server side, but currently has no contained actual CTPs on the server side). This indicates that the FTP supports IM (Inverse Multiplexing) but the IM function is not active and the TCP within the FTP is available for external SNC/crossconnect connectivity.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PublicAccess | Containment | Unspecified
Static | No | Derived | No