Operation void performMaintenanceOperation (CurrentMaintenanceOperation maintenanceOperation = NA, MaintenanceOperationMode maintenanceOperationMode = NA), in Class TerminationPoint

Documentation
Performs maintenance commands.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS dos not supported this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when any input parameter is syntactically incorrect (e.g. maintenanceOperation
is invalid).
4. UNABLE_TO_COMPLY - Raised when the operation is denied by the managed element (e.g. because of the
current state of the object).
5. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
If a command was enabled the maintenace operation is now persistent.
Semantics

Arguments

maintenanceOperation
/* in */ Information on the maintenance operation to perform.
maintenanceOperationMode
/* in */ Indicates whether the maintenance operation should be operated or released.