Indicates whether the EMS supports the launchGCT operation to launch the GCT on the server-side. If this value is false the launch can only be carried out outside the NMS-EMS interface (i.e. a "client-launch")

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
