Requests that the specified (NMS-provided) transmission parameters be set/changed to the specified (NMS-provided) values.
Used, for example, to change path trace parameters on CTPs.
Used, for example, to change parameters such as frame format or line code on PTPs.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when any value of transmissionParameter is syntactically incorrect and raised when a parameter is
    identified as only "settable" using a "specific operation" in the associated supporting document LayeredParameters.pdf;
    i.e. the whole list of parameters will be rejected if one of the parameters indicates that it should be set via a specific operation
    other than setTransmissionParameters.
3. UNABLE_TO_COMPLY - Raised when the EMS is unable to execute the request because at least one of the parameters
    although valid can not be set and that parameter is identified as "not best effort" in the associated supporting document
    LayeredParameters.pdf; i.e. the whole list of parameters will be rejected if one fails that must be set. This is potentially usable
    for cases where two parameters interact and must both be set at once for the operation to be valid.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.
