tmf854.v1 > ProtectionSwitch_T > protectedTP
LOCATION: file:/xsd/networkResources/Notifications.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The protectedTP Element
Identifies the TP that was protected when the switch occurred. For an SNCP, this is always the reliable TP. For a 2F BLSR ring switch notification, this is the TP that is/was inactive during the switch. For a 4FMSSP ring switch notification, this is the worker TP that is/was inactive during the switch. For a 1:N MSP switch notification, this is the worker TP for which the protection switch occurred. For a revertive 1+1 MSP, this is always the worker TP. For a non-revertive 1+1 MSP switch notification, this is the TP that was active before the switch (note that after the switch the protected TP changes).
Element ProtectionSwitch_T/protectedTP : NamingAttributes_T [1 .. 1]
The protectedTP element cannot have "xsi:nil" as an attribute. The protectedTP element in XML instance can be substituted with other elements.

XML Instance
Identifies the TP that was protected when the switch occurred. For an SNCP, this is always the reliable TP. For a 2F BLSR ring switch notification, this is the TP that is/was inactive during the switch. For a 4FMSSP ring switch notification, this is the worker TP that is/was inactive during the switch. For a 1:N MSP switch notification, this is the worker TP for which the protection switch occurred. For a revertive 1+1 MSP, this is always the worker TP. For a non-revertive 1+1 MSP switch notification, this is the TP that was active before the switch (note that after the switch the protected TP changes). <protectedTP extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T"> -Begin Sequence [1...1] Os Name <osNm>NameValue_T</osNm> [0..1] Management Domain name <mdNm>NameValue_T</mdNm> [0..1] Managed Element name <meNm>NameValue_T</meNm> [0..1] Equipment Holder name <ehNm>NameValue_T</ehNm> [0..1] Equipment name <eqNm>NameValue_T</eqNm> [0..1] PTP name <ptpNm>NameValue_T</ptpNm> [0..1] FTP name <ftpNm>NameValue_T</ftpNm> [0..1] CTP name <ctpNm>NameValue_T</ctpNm> [0..1] TPool name <tppoolNm>NameValue_T</tppoolNm> [0..1] Protection Group name <pgpNm>NameValue_T</pgpNm> [0..1] Equipment Protection Group name <epgpNm>NameValue_T</epgpNm> [0..1] MultiLayer Subnetwork name <mlsnNm>NameValue_T</mlsnNm> [0..1] Subnetwork Connection name <sncNm>NameValue_T</sncNm> [0..1] Tranmission Descriptor component of hierarchical name <tmdNm>NameValue_T</tmdNm> [0..1] Topological Link component of hierarchical name. <tlNm>NameValue_T</tlNm> [0..1] AID component of hierarchical name. <aidNm>NameValue_T</aidNm> [0..1] Proprietary vendor object component of hierarchical name. <propNm>NameValue_T</propNm> [0..1] End Sequence </protectedTP>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element name="protectedTP" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> Identifies the TP that was protected when the switch occurred. For an SNCP, this is always the reliable TP. For a 2F BLSR ring switch notification, this is the TP that is/was inactive during the switch. For a 4FMSSP ring switch notification, this is the worker TP that is/was inactive during the switch. For a 1:N MSP switch notification, this is the worker TP for which the protection switch occurred. For a revertive 1+1 MSP, this is always the worker TP. For a non-revertive 1+1 MSP switch notification, this is the TP that was active before the switch (note that after the switch the protected TP changes). </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) NamingAttributes_T

Used-By

Generated by WSDLdoc ©