tmf854.v1 > SubnetworkConnection_T > sncState
LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The sncState Element
The sncState is an attribute managed by the EMS. The EMS manages the state transition of this attribute. The EMS will assess the cross-connections in the network that support the SNC and will appropriately adjust the value of SNCState to reflect the actual state of the SNC in the network.
Element SubnetworkConnection_T/sncState : SNCState_T [0 .. 1]
The sncState element can have "xsi:nil" as an attribute. The sncState element in XML instance can be substituted with other elements.

XML Instance
The sncState is an attribute managed by the EMS. The EMS manages the state transition of this attribute. The EMS will assess the cross-connections in the network that support the SNC and will appropriately adjust the value of SNCState to reflect the actual state of the SNC in the network. <sncState>SNCState_T</sncState>

﻿

Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element minOccurs="0" name="sncState" nillable="true" type="SNCState_T"> -<xsd:annotation> <xsd:documentation> The sncState is an attribute managed by the EMS. The EMS manages the state transition of this attribute. The EMS will assess the cross-connections in the network that support the SNC and will appropriately adjust the value of SNCState to reflect the actual state of the SNC in the network. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) SNCState_T

Used-By

Generated by WSDLdoc ©