The conformance definition for the traffic descriptor from UNI 4.1, UNI 4.0 and UNI 3.1 standards.
For ATM, see attached document for the valid values of this attribute.
This field is nullable if the conformance definition does not apply.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
