The CTP(s) to terminate the one end of the connection (e.g., multiple CTPs may be
specified to support open ring topology or DCS on two UPSRs) specified by NMS in request.
Changes in this rellationship lead to a AVC notification issued by the SNC object.
