tmf854.v1 > ProtectionSwitch_T > switchToTP
LOCATION: file:/xsd/networkResources/Notifications.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The switchToTP Element
Identifies the TP which is being switched to. This identifies the TP that is the active source after the switch, or currently active if no protection switch is currently active. For a 2F BLSR, when the state returns to normal, this is the TP that had switched. For a 4F BLSR ring switch, when the state returns to normal, this is the worker TP of the span that had switched; for example, if the East span had switched to the West span, then this is the East worker TP.
Element ProtectionSwitch_T/switchToTP : NamingAttributes_T [1 .. 1]
The switchToTP element cannot have "xsi:nil" as an attribute. The switchToTP element in XML instance can be substituted with other elements.

XML Instance
Identifies the TP which is being switched to. This identifies the TP that is the active source after the switch, or currently active if no protection switch is currently active. For a 2F BLSR, when the state returns to normal, this is the TP that had switched. For a 4F BLSR ring switch, when the state returns to normal, this is the worker TP of the span that had switched; for example, if the East span had switched to the West span, then this is the East worker TP. <switchToTP extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T"> -Begin Sequence [1...1] Os Name <osNm>NameValue_T</osNm> [0..1] Management Domain name <mdNm>NameValue_T</mdNm> [0..1] Managed Element name <meNm>NameValue_T</meNm> [0..1] Equipment Holder name <ehNm>NameValue_T</ehNm> [0..1] Equipment name <eqNm>NameValue_T</eqNm> [0..1] PTP name <ptpNm>NameValue_T</ptpNm> [0..1] FTP name <ftpNm>NameValue_T</ftpNm> [0..1] CTP name <ctpNm>NameValue_T</ctpNm> [0..1] TPool name <tppoolNm>NameValue_T</tppoolNm> [0..1] Protection Group name <pgpNm>NameValue_T</pgpNm> [0..1] Equipment Protection Group name <epgpNm>NameValue_T</epgpNm> [0..1] MultiLayer Subnetwork name <mlsnNm>NameValue_T</mlsnNm> [0..1] Subnetwork Connection name <sncNm>NameValue_T</sncNm> [0..1] Tranmission Descriptor component of hierarchical name <tmdNm>NameValue_T</tmdNm> [0..1] Topological Link component of hierarchical name. <tlNm>NameValue_T</tlNm> [0..1] AID component of hierarchical name. <aidNm>NameValue_T</aidNm> [0..1] Proprietary vendor object component of hierarchical name. <propNm>NameValue_T</propNm> [0..1] End Sequence </switchToTP>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element name="switchToTP" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> Identifies the TP which is being switched to. This identifies the TP that is the active source after the switch, or currently active if no protection switch is currently active. For a 2F BLSR, when the state returns to normal, this is the TP that had switched. For a 4F BLSR ring switch, when the state returns to normal, this is the worker TP of the span that had switched; for example, if the East span had switched to the West span, then this is the East worker TP. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) NamingAttributes_T

Used-By

Generated by WSDLdoc ©