The ATM Service Category relates quality requirements and traffic characteristics to network behavior (procedures and parameters). It is intended to specify a combination of Quality of Service (QoS) commitment and traffic parameters that is suitable for a given set of applications (user interpretation) and that allows for specific multiplexing schemes at the ATM layer (network interpretation).

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
