CIS CharacterString conformanceDefn = empty string, in Class TrafficDescriptor

Documentation
This attribute specifies the conformance definition which characterizes an ATM Connection. The conformance definitions are from the ATM Forum UNI 4.1, UNI 4.0, and UNI 3.1 standards.
The values are CBR.L1, CBR.L2, VBR.L1, VBR.L2, VBR.L3, VBR.L4, VBR.1, VBR.2, VBR.3, UBR.1, UBR.2, GFR.1, GFR.2, and USER.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No