tmf854.v1 > NetworkRouted_T LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The NetworkRouted_T Simple Type
Network routed, indicates if the route must be or is computed and implemented at the network level. NR_YES indicates that the route must be / is computed at the network. NR_NO indicates that the route must not be / is not computed at the network. NR_NA indicates that the route can be computed anywhere. If rerouting is allowed, this attribute will indicate who last rerouted the SNC, the network (NR_YES) or the EMS (NR_NO).
Simple Type NetworkRouted_T
NetworkRouted_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (NR_NA | NR_NO | NR_YES).

Enumeration | Description
NR_NA |
NR_NO |
NR_YES |

XML
-<xsd:simpleType name="NetworkRouted_T"> -<xsd:annotation> <xsd:documentation> Network routed, indicates if the route must be or is computed and implemented at the network level. NR_YES indicates that the route must be / is computed at the network. NR_NO indicates that the route must not be / is not computed at the network. NR_NA indicates that the route can be computed anywhere. If rerouting is allowed, this attribute will indicate who last rerouted the SNC, the network (NR_YES) or the EMS (NR_NO). </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="NR_NA" /> <xsd:enumeration value="NR_NO" /> <xsd:enumeration value="NR_YES" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) SubnetworkConnection_T/networkRouted

Generated by WSDLdoc ©