Name protectedTP = NA, in Class ProtectionSwitch

Documentation
This is the TP that is protected.
- For a SNCP, this is always the reliable TP.
- For a 2F BLSR ring switch notification, this is the TP that is/was inactive during the switch.
- For a 4FMSSP ring switch notification, this is the worker TP that is/was inactive during the switch.
- For a 1:N trail protection (e.g. MSP) switch notification, this is the worker TP for which the protection switch occurred.
- For a revertive 1+1 trail protection (e.g. MSP) switch notification, this is always the worker TP.
- For a non-revertive 1+1 trail protection (e.g. MSP) switch notification, this is the TP that was active before the switch (note that after the switch the protected TP changes).
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No