Operation void getContainedInUseCTPs (CIS SequenceOf Enums::LayerRate layerRateList = empty list, CIS SequenceOf ConnectionTerminationPoint ctps = NA), in Class TerminationPoint

Documentation
This operation is used to retrieve the "in use" CTPs that are contained within a specific PTP or CTP, at specific layer rates. An "in use" CTP is defined as a CTP that is used by an SNC in any state (including pending), either as a CM end point or as an intermediate connection point, or a CTP that is terminated and mapped. This operation will be used when there are a large number of potential CTPs (e.g., in ATM).
Examples for contained InUse TPs in different states of usage are contained in the associated supporting document ContainedTPs.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when layerRateList contains undefined rates.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
External Documents

SD1-6_ContainedTPs.pdf |

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

layerRateList
/* in */ The list of rates of the contained in-use CTPs to be returned. An empty list indicates to the EMS to get all contained in use CTPs (for all rates).
ctps
/* out */ Complete CTP object(s) for any contained CTP(s).