Operation void getAssociatedTPs (CIS SequenceOf TerminationPoint tps = NA), in Class TransmissionDescriptor

Documentation
The operation retrieves the set of TPs that are associated with this TransmissionDescriptor.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

tps
/* out */ A set of TPs associated with this Transmission Descriptor.