tmf854.v1 > ProposedRepairActionList_T LOCATION: file:/xsd/networkResources/Notifications.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The ProposedRepairActionList_T Complex Type
List of ProposedRepairAction_T elements. The optional "X.733::ProposedRepairActions" parameter uses this type. When present in an alarm notification, it indicates if the cause is known and the system being managed can suggest one or more solutions (such as switch in standby equipment, retry, replace media). This is consistent with the ITU-T X.733 definition.

Local elements (1)
  proposedRepairAction

Complex Type ProposedRepairActionList_T
The ProposedRepairActionList_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<...> <proposedRepairAction>ProposedRepairAction_T</proposedRepairAction> [0..*] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:complexType name="ProposedRepairActionList_T"> -<xsd:annotation> <xsd:documentation> List of ProposedRepairAction_T elements. The optional "X.733::ProposedRepairActions" parameter uses this type. When present in an alarm notification, it indicates if the cause is known and the system being managed can suggest one or more solutions (such as switch in standby equipment, retry, replace media). This is consistent with the ITU-T X.733 definition. </xsd:documentation> </xsd:annotation> -<xsd:sequence> <xsd:element maxOccurs="unbounded" minOccurs="0" name="proposedRepairAction" type="ProposedRepairAction_T" /> </xsd:sequence> </xsd:complexType>

﻿

Uses
Type (1) ProposedRepairAction_T

Used-By
Element (1) Alarm_T/X733_ProposedRepairActions

Generated by WSDLdoc ©