SwitchReason switchReason = NA, in Class SwitchData

Documentation
The reason the last switch occurred. During a switch notification the switch reason is known. If it is not cached in the EMS for later retrieval, then a NA value is assigned.
- The manual switch indicates that a manual operation caused this switch, including MANUAL, FORCED and LOCKOUT switches.
- The AUTOMATIC_SWITCH is used when the switch reason for the automatic switch is not known.
- SIGNAL_MISMATCH is used in the case the signal is ok, but is identified as coming from an incorrect source: TRAIL_TRACE_IDENTIFIER_MISMATCH, Signal Label Mismatch, etc.
- NA is used upon retrieval of switch data for non-revertive groups, if a more precise value is not available.
- RESTORED is used for revertive groups to indicate a return to the normal state.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No