Operation void getAssociatedCTPs (CIS SequenceOf ConnectionTerminationPoint ctps = NA), in Class TrafficDescriptor

Documentation
Get a set of CTPs that are associated with the Traffic Descriptor.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to the ME is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

ctps
/* out */ A set of CTPs associated with this Traffic Descriptor.