tmf854.v1 > PGPParameters_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The PGPParameters_T Complex Type
The definition of the list of PGP parameters. It should be noted that although the term MSP was chosen as the original specific protection scheme to which the related behaviour applied was Multiplex Section Protection, the label is now more generally applied to any 1+1 or 1:N Trail protection scheme. PG type "1+1 trail protection" refers to ProtectionGroupType "MSP_1_PLUS_1", PG type "1:N trail protection" refers to ProtectionGroupType "MSP_1_FOR_N", PG type "2-F MSSPRING" refers to ProtectionGroupType "2_FIBER_BLSR", PG type "2-F MSSPRING" refers to ProtectionGroupType "4_FIBER_BLSR".

Local elements (17)
  SwitchMode SPRINGProtocol SPRINGNodeId SwitchPosition NonPreEmptibleTraffic WtrTime HoldOffTime LODNumSwitches LODDuration TandemSwitching BundleSwitching Hitless ExerciseOn AvailabilityStatus SwitchCriteriaEnable PrivilegedChannel vendorExtensions

Complex Type PGPParameters_T
The PGPParameters_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> -Begin All [1...1] <SwitchMode>SwitchMode_T</SwitchMode> [0..1] <SPRINGProtocol>SPRINGProtocol_T</SPRINGProtocol> [0..1] <SPRINGNodeId>SPRINGNodeId_T</SPRINGNodeId> [0..1] <SwitchPosition>SwitchPosition_T</SwitchPosition> [0..1] <NonPreEmptibleTraffic>NonPreEmptibleTraffic_T</NonPreEmptibleTraffic> [0..1] <WtrTime>WtrTime_T</WtrTime> [0..1] <HoldOffTime>HoldOffTime_T</HoldOffTime> [0..1] <LODNumSwitches>LODNumSwitches_T</LODNumSwitches> [0..1] <LODDuration>LODDuration_T</LODDuration> [0..1] <TandemSwitching>TandemSwitching_T</TandemSwitching> [0..1] <BundleSwitching>BundleSwitching_T</BundleSwitching> [0..1] <Hitless>Hitless_T</Hitless> [0..1] <ExerciseOn>ExerciseOn_T</ExerciseOn> [0..1] <AvailabilityStatus>AvailabilityStatus_T</AvailabilityStatus> [0..1] <SwitchCriteriaEnable>SwitchCriteriaEnable_T</SwitchCriteriaEnable> [0..1] <PrivilegedChannel>PrivilegedChannel_T</PrivilegedChannel> [0..1] <vendorExtensions extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T">PGPParametersExt_T</vendorExtensions> [0..1] End All </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="PGPParameters_T"> -<xsd:annotation> <xsd:documentation> The definition of the list of PGP parameters. It should be noted that although the term MSP was chosen as the original specific protection scheme to which the related behaviour applied was Multiplex Section Protection, the label is now more generally applied to any 1+1 or 1:N Trail protection scheme. PG type "1+1 trail protection" refers to ProtectionGroupType "MSP_1_PLUS_1", PG type "1:N trail protection" refers to ProtectionGroupType "MSP_1_FOR_N", PG type "2-F MSSPRING" refers to ProtectionGroupType "2_FIBER_BLSR", PG type "2-F MSSPRING" refers to ProtectionGroupType "4_FIBER_BLSR". </xsd:documentation> </xsd:annotation> -<xsd:all> <xsd:element minOccurs="0" name="SwitchMode" type="SwitchMode_T" /> <xsd:element minOccurs="0" name="SPRINGProtocol" type="SPRINGProtocol_T" /> <xsd:element minOccurs="0" name="SPRINGNodeId" type="SPRINGNodeId_T" /> <xsd:element minOccurs="0" name="SwitchPosition" type="SwitchPosition_T" /> <xsd:element minOccurs="0" name="NonPreEmptibleTraffic" type="NonPreEmptibleTraffic_T" /> <xsd:element minOccurs="0" name="WtrTime" type="WtrTime_T" /> <xsd:element minOccurs="0" name="HoldOffTime" type="HoldOffTime_T" /> <xsd:element minOccurs="0" name="LODNumSwitches" type="LODNumSwitches_T" /> <xsd:element minOccurs="0" name="LODDuration" type="LODDuration_T" /> <xsd:element minOccurs="0" name="TandemSwitching" type="TandemSwitching_T" /> <xsd:element minOccurs="0" name="BundleSwitching" type="BundleSwitching_T" /> <xsd:element minOccurs="0" name="Hitless" type="Hitless_T" /> <xsd:element minOccurs="0" name="ExerciseOn" type="ExerciseOn_T" /> <xsd:element minOccurs="0" name="AvailabilityStatus" type="AvailabilityStatus_T" /> <xsd:element minOccurs="0" name="SwitchCriteriaEnable" type="SwitchCriteriaEnable_T" /> <xsd:element minOccurs="0" name="PrivilegedChannel" type="PrivilegedChannel_T" /> <xsd:element minOccurs="0" name="vendorExtensions" type="PGPParametersExt_T" /> </xsd:all> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (19) AvailabilityStatus_T BundleSwitching_T ExerciseOn_T Hitless_T HoldOffTime_T LODDuration_T LODNumSwitches_T NonPreEmptibleTraffic_T PGPParametersExt_T PrivilegedChannel_T SPRINGNodeId_T SPRINGProtocol_T string SwitchCriteriaEnable_T SwitchMode_T SwitchPosition_T TandemSwitching_T TMF854_Version_T WtrTime_T

Used-By
Element (1) ProtectionGroup_T/pgpParameters

Generated by WSDLdoc ©