Name switchToTP = NA, in Class ProtectionSwitch

Documentation
Identifies the TP which is being switched to. This identifies the TP that is the active source after the switch.
For a 2F BLSR, when the state returns to normal, this is the TP that had switched.
For a 4F BLSR ring switch, when the state returns to normal, this is the worker TP of the span that had switched; for example, if the East span had switched to the West span, then this is the East worker TP.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No