Association (transmissionParameters:TransmissionParameters) (theTerminationPoint:TerminationPoint)

Documentation
A list of transmission parameters per layer rate which can be set and/or retrieved on the TP. This attribute must contain the complete set of layer rates represented by a PTP or CTP - even if they have no parameters associated with them.
The following rule will allow the NMS to figure out the relationships between the containing/contained TPs:
- When a contained TP is the client of its containing TP (usual case), no layer should be repeated in the two TPs.
- When a contained TP is not the client of its containing TP, the layer that links the containing and contained TPs must be repeated in both TPs.
The layers of a TP are listed starting with the server-most layer; each layer is then followed by its client layer(s).
The server-most layer of a PTPs is always its physical layer. For FTPs and CTPs, it could be any layer.
When there are optional layers in a TP, the server-client relationships used to construct the layer order only
considers active layers (as indicated by the ThisLayerActive transmission parameter). The order chosen for
the complete list of layers (including active and inactive layers) must remain valid for every possible combination
of ThisLayerActive values. This usually results in more than one valid order.

Derived | No | Link Class | --Not Defined--
Element 1 | TransmissionParameters | Element 2 | TerminationPoint
Role 1 | transmissionParameters | Role 2 | --Not Named--