Operation void getAssociatedTP (Name tpName = NA, CIS SequenceOf TerminationPoint associatedTPs = NA), in Class MultiLayerSubnetwork

Documentation
This operation returns a list of PSR (UPSR or SNCP) associated termination points for the TP whose name is passed as a parameter.
The operation allows the NMS to query the associated CTP of a given CTP or associated PTP given a PTP. The timeslot of the TPs will be the same in the case of an OPEN_PSR subnetwork, but the names of the two TPs will be different.
This operation is symmetric on the associated TPs. Given a working TP, the associated TP will be the protecting TP.
When this operation is invoked with a TP that is not an edge point, the returned TPs will be on the same Managed Element.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS cannot support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when tpName does not reference a CTP or PTP.
4. ENTITY_NOT_FOUND - Raised when tpName references a CTP or PTP object that does not exist.
5. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
Identified TP has to exist.
Postconditions
No change in the system.
Semantics

Arguments

tpName
/* in */ The name of the TP for which the associated TP(s) are requested.
associatedTPs
/* out */ The PSR associated TPs. If there are no PSR associated TPs, then an empty list is returned..