Class TransmissionParameters {Analysis}

Documentation
A list of transmission parameters per layer rate which can be set and/or retrieved on the TP.
Note: Setting is prohibited for some specific parameters.
This object can be set by an NMS through the ME.setTPData() and also during SNC creation.
Object Lifecycle: Lifecycle tied to TP.
Object Creation Notification Issued? NA
Object Deletion Notification Issued? NA
External Documents

SD1-16_LayeredParameters.pdf |

Parent Package | Logical View | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Operations

Name | Signature | Class
setTransmissionParameters | void setTransmissionParameters (CIS SequenceOf Structs::AVP transmissionParameters = NA) | TransmissionParameters

Attributes

Name | Class | Type | Initial Value
layerRate | TransmissionParameters | LayerRate | NA
transmissionParameters | TransmissionParameters | CIS SequenceOf Structs::AVP | NA

Associations

Name | My Role | My Class | Other Role | Other Element
--Not Named-- | transmissionParameters | TransmissionParameters | --Not Named-- | TerminationPoint
--Not Named-- | transmissionParameters | TransmissionParameters | --Not Named-- | TPData
--Not Named-- | transmissionParameters | TransmissionParameters | --Not Named-- | TransmissionDescriptorCreateData
--Not Named-- | transmissionParameters | TransmissionParameters | --Not Named-- | TransmissionDescriptor