tmf854.v1 > LODNumSwitches_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The LODNumSwitches_T Simple Type
LODNumSwitches and LODDuration are used together to specify when Lock Out should occur. If the specified number of switches occur within the specified duration, the result is Lock Out for that group.
<ApplicableTo>For non-revertive switches. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo>
Simple Type LODNumSwitches_T
LODNumSwitches_T is derived from unsignedInt type. There are several restrictions on the value. The range of the value is [0..4294967295]. The schema processor collapses value's whitespace. The number of fractional digits is less than or equals to 0.

XML
-<xsd:simpleType name="LODNumSwitches_T"> -<xsd:annotation> -<xsd:documentation> LODNumSwitches and LODDuration are used together to specify when Lock Out should occur. If the specified number of switches occur within the specified duration, the result is Lock Out for that group. <ApplicableTo>For non-revertive switches. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo> </xsd:documentation> </xsd:annotation> <xsd:restriction base="xsd:unsignedInt"> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) unsignedInt

Used-By
Element (1) PGPParameters_T/LODNumSwitches

Generated by WSDLdoc ©